{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Лист1"],"not_rendered":{"charts":1,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Лист1","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[]}
["Расчет грунтового откоса на устойчивость по методу круглоцилиндрических поверхностей"]
[null,"Задать числовые параметры",null,null,"Результаты расчета"]
[null,"и нажать \"Рассчитать\"",null,null,"Время счета не более 15 секунд"]
["h =",3,"м","m =",0.4127679844594227]
["γ =",16,"кН/м3","Xc =",-2.0363905273452696,"м"]
["c =",5,"кН/м2","Yc =",4.1377082758364514,"м"]
["ϕ =",23,"◦","R =",4.6116717311390456,"м"]
["q =",4,"кН/м2","a =",0,"м"]
["bf =",1.35,"м","b =",1.1944369824223218,"м"]
["Kn =",1,null,"Кmin =",1.0000000024602895]
[]
[]
[null,"Построение профиля откоса и призмы обрушения"]
["Xоткос","Yоткос","Xокружн","Yокружн"]
[{"$f":"-(E8+E9)","v":-1.1944369824223218},0,0,0]
[0,0,0.24327409358005897,0.12888733048501511]
[{"$f":"E4*B4","v":1.238303953378268},{"$f":"B4","v":3},0.48654818716011794,0.27735901720234368]
[{"$f":"E4*B4+B9+1.5*E9","v":4.3799594270117508},{"$f":"B4","v":3},0.72982228074017685,0.44777835019138124]
[null,null,0.97309637432023588,0.64335501028204289]
[null,null,1.2163704679002949,0.86860104853476994]
["Xq","Yq",1.4596445614803537,1.1301752646315837]
[{"$f":"E4*B4+B9","v":2.5883039533782681},{"$f":"B4","v":3},1.7029186550604127,1.438618986064149]
[{"$f":"E4*B4+B9","v":2.5883039533782681},{"$f":"1.1*B4","v":3.3000000000000003},1.9461927486404718,1.8125100895250816]
[{"$f":"E4*B4+B9+1.5*E9","v":4.3799594270117508},{"$f":"1.1*B4","v":3.3000000000000003},2.1894668422205306,2.2911856932847456]
[{"$f":"E4*B4+B9+1.5*E9","v":4.3799594270117508},{"$f":"B4","v":3},2.4327409358005898,3]